The graph below shows BW/Latency from Idle to max efficiency of a specific config. It was generated on DMR pre-sim MC IP model using TIE traffic with latency and BW efficiency numbers captured using only PMON data.

A graph with a line graph

Description automatically generated